X-Git-Url: https://git.saurik.com/wxWidgets.git/blobdiff_plain/c94f845b1602d44ccd7c7542afffde666adbb2f0..a607d8d633e055fc5cea22c0b829cd65b5c3dbfb:/docs/latex/wx/dc.tex

diff --git a/docs/latex/wx/dc.tex b/docs/latex/wx/dc.tex
index c8d929e22a..0c7b36cc80 100644
--- a/docs/latex/wx/dc.tex
+++ b/docs/latex/wx/dc.tex
@@ -32,6 +32,10 @@ the color's alpha values when stroking or filling.
 
 <wx/dc.h>
 
+\wxheading{Library}
+
+\helpref{wxCore}{librarieslist}
+
 \wxheading{See also}
 
 \helpref{Overview}{dcoverview}
@@ -199,7 +203,7 @@ See also \helpref{wxDC::SetClippingRegion}{wxdcsetclippingregion}.
 
 \membersection{wxDC::DeviceToLogicalX}\label{wxdcdevicetologicalx}
 
-\func{wxCoord}{DeviceToLogicalX}{\param{wxCoord}{ x}}
+\func{virtual wxCoord}{DeviceToLogicalX}{\param{wxCoord}{ x}}
 
 Convert device X coordinate to logical coordinate, using the current
 mapping mode.
@@ -207,7 +211,7 @@ mapping mode.
 
 \membersection{wxDC::DeviceToLogicalXRel}\label{wxdcdevicetologicalxrel}
 
-\func{wxCoord}{DeviceToLogicalXRel}{\param{wxCoord}{ x}}
+\func{virtual wxCoord}{DeviceToLogicalXRel}{\param{wxCoord}{ x}}
 
 Convert device X coordinate to relative logical coordinate, using the current
 mapping mode but ignoring the x axis orientation.
@@ -216,7 +220,7 @@ Use this function for converting a width, for example.
 
 \membersection{wxDC::DeviceToLogicalY}\label{wxdcdevicetologicaly}
 
-\func{wxCoord}{DeviceToLogicalY}{\param{wxCoord}{ y}}
+\func{virtual wxCoord}{DeviceToLogicalY}{\param{wxCoord}{ y}}
 
 Converts device Y coordinate to logical coordinate, using the current
 mapping mode.
@@ -224,7 +228,7 @@ mapping mode.
 
 \membersection{wxDC::DeviceToLogicalYRel}\label{wxdcdevicetologicalyrel}
 
-\func{wxCoord}{DeviceToLogicalYRel}{\param{wxCoord}{ y}}
+\func{virtual wxCoord}{DeviceToLogicalYRel}{\param{wxCoord}{ y}}
 
 Convert device Y coordinate to relative logical coordinate, using the current
 mapping mode but ignoring the y axis orientation.
@@ -880,7 +884,7 @@ use \arg{initialColour} on the left part of the rectangle and
 
 \membersection{wxDC::LogicalToDeviceX}\label{wxdclogicaltodevicex}
 
-\func{wxCoord}{LogicalToDeviceX}{\param{wxCoord}{ x}}
+\func{virtual wxCoord}{LogicalToDeviceX}{\param{wxCoord}{ x}}
 
 Converts logical X coordinate to device coordinate, using the current
 mapping mode.
@@ -888,7 +892,7 @@ mapping mode.
 
 \membersection{wxDC::LogicalToDeviceXRel}\label{wxdclogicaltodevicexrel}
 
-\func{wxCoord}{LogicalToDeviceXRel}{\param{wxCoord}{ x}}
+\func{virtual wxCoord}{LogicalToDeviceXRel}{\param{wxCoord}{ x}}
 
 Converts logical X coordinate to relative device coordinate, using the current
 mapping mode but ignoring the x axis orientation.
@@ -897,7 +901,7 @@ Use this for converting a width, for example.
 
 \membersection{wxDC::LogicalToDeviceY}\label{wxdclogicaltodevicey}
 
-\func{wxCoord}{LogicalToDeviceY}{\param{wxCoord}{ y}}
+\func{virtual wxCoord}{LogicalToDeviceY}{\param{wxCoord}{ y}}
 
 Converts logical Y coordinate to device coordinate, using the current
 mapping mode.
@@ -905,7 +909,7 @@ mapping mode.
 
 \membersection{wxDC::LogicalToDeviceYRel}\label{wxdclogicaltodeviceyrel}
 
-\func{wxCoord}{LogicalToDeviceYRel}{\param{wxCoord}{ y}}
+\func{virtual wxCoord}{LogicalToDeviceYRel}{\param{wxCoord}{ y}}
 
 Converts logical Y coordinate to relative device coordinate, using the current
 mapping mode but ignoring the y axis orientation.
