X-Git-Url: https://git.saurik.com/wxWidgets.git/blobdiff_plain/e3b81044ee30ead362ba6e1bf95af13248afe41c..e31f4da5f0e888e3bae947061be02a427c570372:/docs/latex/wx/dc.tex

diff --git a/docs/latex/wx/dc.tex b/docs/latex/wx/dc.tex
index cffeac284a..e5ce0687ed 100644
--- a/docs/latex/wx/dc.tex
+++ b/docs/latex/wx/dc.tex
@@ -199,7 +199,7 @@ See also \helpref{wxDC::SetClippingRegion}{wxdcsetclippingregion}.
 
 \membersection{wxDC::DeviceToLogicalX}\label{wxdcdevicetologicalx}
 
-\func{wxCoord}{DeviceToLogicalX}{\param{wxCoord}{ x}}
+\func{virtual wxCoord}{DeviceToLogicalX}{\param{wxCoord}{ x}}
 
 Convert device X coordinate to logical coordinate, using the current
 mapping mode.
@@ -207,7 +207,7 @@ mapping mode.
 
 \membersection{wxDC::DeviceToLogicalXRel}\label{wxdcdevicetologicalxrel}
 
-\func{wxCoord}{DeviceToLogicalXRel}{\param{wxCoord}{ x}}
+\func{virtual wxCoord}{DeviceToLogicalXRel}{\param{wxCoord}{ x}}
 
 Convert device X coordinate to relative logical coordinate, using the current
 mapping mode but ignoring the x axis orientation.
@@ -216,7 +216,7 @@ Use this function for converting a width, for example.
 
 \membersection{wxDC::DeviceToLogicalY}\label{wxdcdevicetologicaly}
 
-\func{wxCoord}{DeviceToLogicalY}{\param{wxCoord}{ y}}
+\func{virtual wxCoord}{DeviceToLogicalY}{\param{wxCoord}{ y}}
 
 Converts device Y coordinate to logical coordinate, using the current
 mapping mode.
@@ -224,7 +224,7 @@ mapping mode.
 
 \membersection{wxDC::DeviceToLogicalYRel}\label{wxdcdevicetologicalyrel}
 
-\func{wxCoord}{DeviceToLogicalYRel}{\param{wxCoord}{ y}}
+\func{virtual wxCoord}{DeviceToLogicalYRel}{\param{wxCoord}{ y}}
 
 Convert device Y coordinate to relative logical coordinate, using the current
 mapping mode but ignoring the y axis orientation.
@@ -793,7 +793,7 @@ Gets the current text background colour (see \helpref{wxDC::SetTextBackground}{w
 \membersection{wxDC::GetTextExtent}\label{wxdcgettextextent}
 
 \constfunc{void}{GetTextExtent}{\param{const wxString\& }{string}, \param{wxCoord *}{w}, \param{wxCoord *}{h},\\
-  \param{wxCoord *}{descent = NULL}, \param{wxCoord *}{externalLeading = NULL}, \param{wxFont *}{font = NULL}}
+  \param{wxCoord *}{descent = NULL}, \param{wxCoord *}{externalLeading = NULL}, \param{const wxFont *}{font = NULL}}
 
 \constfunc{wxSize}{GetTextExtent}{\param{const wxString\& }{string}}
 
@@ -880,7 +880,7 @@ use \arg{initialColour} on the left part of the rectangle and
 
 \membersection{wxDC::LogicalToDeviceX}\label{wxdclogicaltodevicex}
 
-\func{wxCoord}{LogicalToDeviceX}{\param{wxCoord}{ x}}
+\func{virtual wxCoord}{LogicalToDeviceX}{\param{wxCoord}{ x}}
 
 Converts logical X coordinate to device coordinate, using the current
 mapping mode.
@@ -888,7 +888,7 @@ mapping mode.
 
 \membersection{wxDC::LogicalToDeviceXRel}\label{wxdclogicaltodevicexrel}
 
-\func{wxCoord}{LogicalToDeviceXRel}{\param{wxCoord}{ x}}
+\func{virtual wxCoord}{LogicalToDeviceXRel}{\param{wxCoord}{ x}}
 
 Converts logical X coordinate to relative device coordinate, using the current
 mapping mode but ignoring the x axis orientation.
@@ -897,7 +897,7 @@ Use this for converting a width, for example.
 
 \membersection{wxDC::LogicalToDeviceY}\label{wxdclogicaltodevicey}
 
-\func{wxCoord}{LogicalToDeviceY}{\param{wxCoord}{ y}}
+\func{virtual wxCoord}{LogicalToDeviceY}{\param{wxCoord}{ y}}
 
 Converts logical Y coordinate to device coordinate, using the current
 mapping mode.
@@ -905,7 +905,7 @@ mapping mode.
 
 \membersection{wxDC::LogicalToDeviceYRel}\label{wxdclogicaltodeviceyrel}
 
-\func{wxCoord}{LogicalToDeviceYRel}{\param{wxCoord}{ y}}
+\func{virtual wxCoord}{LogicalToDeviceYRel}{\param{wxCoord}{ y}}
 
 Converts logical Y coordinate to relative device coordinate, using the current
 mapping mode but ignoring the y axis orientation.
